INFLO Setup Instructions

1. Follow the instructions for installing the mount antenna on the car (see installation instruction sheet stored with the antenna in kit).
2. Attach the antenna’s green connectors to the two blue ports next to each other on side of the Locomate unit (any pairing will work).
3. Attach the antenna’s blue connector to the remaining blue port on the Locomate unit.
4. Plug cigarette lighter to USB adapter into car and Locomate unit to power the unit.

NOTE: Do not power the Locomate unit until after connecting the antenna to the unit. Doing otherwise can cause operation issues.

1. Attach windshield mount for Android smartphone to windshield.
2. Open the INFLO app on the Android smartphone to run application.